Post Production Disinfection

Before sending your 3D printed shields to their final destination they must be disinfected to remove any possible contaminants. Gloves should be worn to prevent recontamination.

* To begin with start by wiping down a bench with a surface disinfectant and allow to dry, put down some paper towels to stop your shields getting damaged.
* Fill a bucket/tub with 10L of warm water, add 30mL of dishwashing liquid and stir to combine
* Wash shields with a clean soft cloth in the soapy water and then rinse off in cold water
* Set down on the paper towels
* Wipe down shields with a paper towel to remove excess water
* Spray with isopropyl alcohol and allow to air dry

Once the shields are dry they are ready to be packaged and sent out to frontline workers.